**INDIAN INSTITUTE OF ENGINEERING SCIENCE AND TECHNOLOGY SHIBPUR, P.O. Botanic Garden (Formerly Bengal Engineering And Science University)**

**HOWRAH (West Bengal, India)-711103**

Phone: 033 26681503, 033 26684561 Fax: 033 26682916

Tender No:-07/DY.REG./19-20 Date:-30.05.2019

**Notice Inviting Tender**

|  |
| --- |
| Sealed quotations are invited from bonafide Contractors for Emergent renovation of east side corner room and corridors adjacent to rooms at Lecture hall complex inside the campus of IIEST, Shibpur, Howrah.The quotation will be received in the drop box at the Office of the Registrar, Purchase section between 11.00 a.m and 5.00 p.m on all working days latest by 07.06.2019. Opening on 08.06.2019 at 1.30 p.m.at the Office of the University Engineer. REGISTRARTerms & conditions:- 1. All rates quoted should be inclusive of all taxes, levies & duties. The rate should be quoted both in figures and words.
2. The work should be executed carefully without damaging existing underground / overhead service lines (Water, Electricity, Sewerage lines)
3. Bidder should visit the site and assume the quantity of the work prior to submission of tender.
4. No advance payment can be made
5. The Order no is to be noted on both Challan & Bill
6. Payment will be made on submission of proper bill, Challan etc., by A/C payee cheque. No cash payment will be made under any circumstances
7. Copies of the PAN Card & GST Registration Certificate and Trade License and Professional TAX Certificate should be attached with the quotation
8. Contractors / Bidders are requested to inspect the site before submitting the quotation.
9. The work should be completed within 15 days after receiving the work-order.
 |

 Dy.Registrar,

( Purchase & Store)

 IIEST Shibpur

Copy forwarded for information and necessary action to:

1. Institute Website,

2. Notice board,

3.University Engineer.

|  |
| --- |
| **Name of the Work: Emergent renovation of east side corner room and corridors adjacent to rooms at Lecture hall complex inside the campus.** |
| Sl No | Description of items of work(Based on PWD schedule of rates w.e.f. 01.11.2017.) | Unit | Unit Rate (Rs) | Quantity/ Size | **Amount (Rupees)** |
|
| 1 | Supplying and laying true to line and level vitrified tiles of approved brand (size not less than 600 mm X 600 mm X 10 mm thick) in floor, skirting etc. set in 20 mm sand cement mortar (1:4) and 2 mm thick cement slurry back side of tiles using cement @ 2.91Kg./sqM or using polymerised adhesive (6 mm thick layer applied directly over finished artificial stone floor/Mosaic etc without any backing course) laid after application slurry using 1.75 Kg of cement per sqM below mortar only, joints grouted with admixture of white cement and colouring pigment to match with colour of tiles / epoxy grout materials of approved make as directed and removal of wax coating of top surface of tiles with warm water and polishing the tiles using soft and dry cloth upto mirror finish complete including the cost of materials, labour and all other incidental charges complete true to the manufacturer'sspecification and direction of Engineer-in-Charge. (White cement, synthetic adhesive and grout material to be suppliedby the contrr]e)( Page 66 , Item 36) | sqm |  |   |   |
|   | (II) With Polymerised Adhesive [6 mm thick] & epoxy grouting materials for filling joints including spacer-2 mm [Applied directly over finished artificial stone floor/ mosaic etc.(B) Light Colour | sqm | 1369.00 | 119.29 | 163308.01 |
|   | east side room | sqm | 1369.00 |   |   |
|   | corridor | sqm | 1369.00 |   |   |
|   | corridor | sqm | 1369.00 |   |   |
| 2 | Dismantling all types of plain cement concrete works, stacking serviceable materials at site and removing rubbish as directed within a lead of 75 m. (a) upto 150 mm. thick( Page 10 , Item 2) | Cum | 939.00 | 3.55 | 3333.45 |
| 3 | Brick work with 1st class bricks in cement mortar (1:6) (a) In foundation and plinth( Page 15 , Item 8) | Cum | 5214.00 | 1.11 | 5787.54 |
| **Total** | **172429.00** |
| **Add GST 12%** | **20691.48** |
| **Add 1% for Labour welfare cess** | **1724.29** |
| Total value of work | 194844.77 |
| **To qualify for award of the contract the bidder: -**(a) should have satisfactorily completed as a prime contractor at least one similar work of value not less than Rs. 1,00,000/- (Rupees one lakh only) **Security Deposit:** The employer shall retain 10% from each payment due to the contractor as security deposit which shall be released when the Period of Maintenance has passed and Engineer has certified that all defects notified by the Engineer to the Contractor before the end of this period have been corrected.**Period of Maintenance.** The “Period of Maintenance” for the work is twelve months from the date of taking over possession of the completed works or one full monsoon season whichever occurs later. During the period of maintenance, the contractor will be responsible for rectifying any defects in construction free of cost to the Employer |
| I / We offer to execute the Works described in the Bill of Quantities in Part II of the Tender Document in your letter / tender no referred to above in accordance with the Conditions of Contract enclosed therewith at \_\_\_\_\_\_\_\_\_\_\_ percentage above / below (\*) the estimated rates, i.e. for a total Contract Price of Rs. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ [in figures] \*Rs. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ [in words]"  Authorized Signature : Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_  |